{ "Info" "IQEXE_SEPARATOR" "" "*******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "Quartus II" 0 -1 1433814835595 ""}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "TimeQuest Timing Analyzer Quartus II 64-Bit " "Running Quartus II 64-Bit TimeQuest Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 13.1.0 Build 162 10/23/2013 SJ Full Version " "Version 13.1.0 Build 162 10/23/2013 SJ Full Version" {  } {  } 0 0 "%1!s!" 0 0 "Quartus II" 0 -1 1433814835596 ""} { "Info" "IQEXE_START_BANNER_TIME" "Tue Jun 09 09:53:55 2015 " "Processing started: Tue Jun 09 09:53:55 2015" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "Quartus II" 0 -1 1433814835596 ""}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "Quartus II" 0 -1 1433814835596 ""}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_sta top -c top " "Command: quartus_sta top -c top" {  } {  } 0 0 "Command: %1!s!" 0 0 "Quartus II" 0 -1 1433814835596 ""}
{ "Info" "0" "" "qsta_default_script.tcl version: #1" {  } {  } 0 0 "qsta_default_script.tcl version: #1" 0 0 "Quartus II" 0 0 1433814835691 ""}
{ "Info" "IQCU_PARALLEL_AUTODETECT_MULTIPLE_PROCESSORS_MORE_LOGICAL" "4 4 8 " "Parallel Compilation has detected 8 hyper-threaded processors. However, the extra hyper-threaded processors will not be used by default. Parallel Compilation will use 4 of the 4 physical processors detected instead." {  } {  } 0 11104 "Parallel Compilation has detected %3!i! hyper-threaded processors. However, the extra hyper-threaded processors will not be used by default. Parallel Compilation will use %1!i! of the %2!i! physical processors detected instead." 0 0 "Quartus II" 0 -1 1433814835875 ""}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "Core supply voltage 1.2V " "Core supply voltage is 1.2V" {  } {  } 0 21077 "%1!s! is %2!s!" 0 0 "Quartus II" 0 -1 1433814835876 ""}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "Low junction temperature 0 degrees C " "Low junction temperature is 0 degrees C" {  } {  } 0 21077 "%1!s! is %2!s!" 0 0 "Quartus II" 0 -1 1433814835929 ""}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "High junction temperature 85 degrees C " "High junction temperature is 85 degrees C" {  } {  } 0 21077 "%1!s! is %2!s!" 0 0 "Quartus II" 0 -1 1433814835929 ""}
{ "Info" "ISTA_SDC_STATEMENT_PARENT" "" "Evaluating HDL-embedded SDC commands" { { "Info" "ISTA_SDC_STATEMENT_ENTITY" "altera_avalon_st_clock_crosser " "Entity altera_avalon_st_clock_crosser" { { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\] " "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\] " "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\] " "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\] " "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\] " "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\] " "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\] " "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\] " "set_false_path -from \[get_registers *altera_avalon_st_clock_crosser:*\|in_data_buffer*\] -to \[get_registers *altera_avalon_st_clock_crosser:*\|out_data_buffer*\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""}  } {  } 0 332165 "Entity %1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_ENTITY" "altera_std_synchronizer " "Entity altera_std_synchronizer" { { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_false_path -to \[get_keepers \{*altera_std_synchronizer:*\|din_s1\}\] " "set_false_path -to \[get_keepers \{*altera_std_synchronizer:*\|din_s1\}\]" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""}  } {  } 0 332165 "Entity %1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_ENTITY" "sld_jtag_hub " "Entity sld_jtag_hub" { { "Info" "ISTA_SDC_STATEMENT_EVAL" "create_clock -name altera_reserved_tck \[get_ports \{altera_reserved_tck\}\] -period 10MHz    " "create_clock -name altera_reserved_tck \[get_ports \{altera_reserved_tck\}\] -period 10MHz   " {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""} { "Info" "ISTA_SDC_STATEMENT_EVAL" "set_clock_groups -asynchronous -group \{altera_reserved_tck\} " "set_clock_groups -asynchronous -group \{altera_reserved_tck\}" {  } {  } 0 332166 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""}  } {  } 0 332165 "Entity %1!s!" 0 0 "Quartus II" 0 -1 1433814836184 ""}  } {  } 0 332164 "Evaluating HDL-embedded SDC commands" 0 0 "Quartus II" 0 -1 1433814836184 ""}
{ "Info" "ISTA_SDC_FOUND" "JTAG_MM/synthesis/submodules/altera_reset_controller.sdc " "Reading SDC File: 'JTAG_MM/synthesis/submodules/altera_reset_controller.sdc'" {  } {  } 0 332104 "Reading SDC File: '%1!s!'" 0 0 "Quartus II" 0 -1 1433814836193 ""}
{ "Info" "ISTA_SDC_FOUND" "JTAG_MM/synthesis/submodules/altera_avalon_st_jtag_interface.sdc " "Reading SDC File: 'JTAG_MM/synthesis/submodules/altera_avalon_st_jtag_interface.sdc'" {  } {  } 0 332104 "Reading SDC File: '%1!s!'" 0 0 "Quartus II" 0 -1 1433814836202 ""}
{ "Warning" "WSTA_NODE_FOUND_WITHOUT_CLOCK_ASSIGNMENT" "CLOCK_50 " "Node: CLOCK_50 was determined to be a clock but was found without an associated clock assignment." {  } {  } 0 332060 "Node: %1!s! was determined to be a clock but was found without an associated clock assignment." 0 0 "Quartus II" 0 -1 1433814836211 "|top|CLOCK_50"}
{ "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_PARENT" "" "The following clock transfers have no clock uncertainty assignment. For more accurate results, apply clock uncertainty assignments or use the derive_clock_uncertainty command." { { "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_CHILD" "altera_reserved_tck (Rise) altera_reserved_tck (Rise) setup and hold " "From altera_reserved_tck (Rise) to altera_reserved_tck (Rise) (setup and hold)" {  } {  } 1 332169 "From %1!s! to %2!s! (%3!s!)" 0 0 "Quartus II" 0 -1 1433814836339 ""} { "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_CHILD" "altera_reserved_tck (Rise) altera_reserved_tck (Fall) setup and hold " "From altera_reserved_tck (Rise) to altera_reserved_tck (Fall) (setup and hold)" {  } {  } 1 332169 "From %1!s! to %2!s! (%3!s!)" 0 0 "Quartus II" 0 -1 1433814836339 ""}  } {  } 1 332168 "The following clock transfers have no clock uncertainty assignment. For more accurate results, apply clock uncertainty assignments or use the derive_clock_uncertainty command." 0 0 "Quartus II" 0 -1 1433814836339 ""}
{ "Info" "0" "" "Found TIMEQUEST_REPORT_SCRIPT_INCLUDE_DEFAULT_ANALYSIS = ON" {  } {  } 0 0 "Found TIMEQUEST_REPORT_SCRIPT_INCLUDE_DEFAULT_ANALYSIS = ON" 0 0 "Quartus II" 0 0 1433814836341 ""}
{ "Info" "0" "" "Analyzing Slow 1200mV 85C Model" {  } {  } 0 0 "Analyzing Slow 1200mV 85C Model" 0 0 "Quartus II" 0 0 1433814836356 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "setup 44.576 " "Worst-case setup slack is 44.576" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836379 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836379 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   44.576               0.000 altera_reserved_tck  " "   44.576               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836379 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814836379 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "hold 0.359 " "Worst-case hold slack is 0.359" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836388 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836388 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    0.359               0.000 altera_reserved_tck  " "    0.359               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836388 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814836388 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "recovery 48.605 " "Worst-case recovery slack is 48.605" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836394 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836394 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   48.605               0.000 altera_reserved_tck  " "   48.605               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836394 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814836394 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "removal 0.894 " "Worst-case removal slack is 0.894" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836398 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836398 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    0.894               0.000 altera_reserved_tck  " "    0.894               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836398 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814836398 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "minimum pulse width 49.629 " "Worst-case minimum pulse width slack is 49.629" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836401 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836401 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   49.629               0.000 altera_reserved_tck  " "   49.629               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836401 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814836401 ""}
{ "Info" "ISTA_REPORT_METASTABILITY_INFO" "Report Metastability: Found 5 synchronizer chains. " "Report Metastability: Found 5 synchronizer chains." { { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst-Case MTBF of Design is 1e+09 years or 3.15e+16 seconds. " "Worst-Case MTBF of Design is 1e+09 years or 3.15e+16 seconds." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Typical MTBF of Design is 1e+09 years or 3.15e+16 seconds.\n " "Typical MTBF of Design is 1e+09 years or 3.15e+16 seconds.\n" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Number of Synchronizer Chains Found: 5 " "Number of Synchronizer Chains Found: 5" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Shortest Synchronizer Chain: 3 Registers " "Shortest Synchronizer Chain: 3 Registers" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Fraction of Chains for which MTBFs Could Not be Calculated: 0.000 " "Fraction of Chains for which MTBFs Could Not be Calculated: 0.000" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst Case Available Settling Time: 198.395 ns " "Worst Case Available Settling Time: 198.395 ns" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" " " "" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst-Case MTBF values are calculated based on the worst-case silicon characteristics, with worst-case operating conditions. " "Worst-Case MTBF values are calculated based on the worst-case silicon characteristics, with worst-case operating conditions." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "  - Under worst-case conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 6.5 " "  - Under worst-case conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 6.5" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Typical MTBF values are calculated based on the nominal silicon characteristics, at nominal operating conditions. " "Typical MTBF values are calculated based on the nominal silicon characteristics, at nominal operating conditions." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "  - Under typical conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 9.9 " "  - Under typical conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 9.9" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""}  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814836495 ""}
{ "Info" "0" "" "Analyzing Slow 1200mV 0C Model" {  } {  } 0 0 "Analyzing Slow 1200mV 0C Model" 0 0 "Quartus II" 0 0 1433814836502 ""}
{ "Info" "ITAPI_TAPI_STARTED" "" "Started post-fitting delay annotation" {  } {  } 0 334003 "Started post-fitting delay annotation" 0 0 "Quartus II" 0 -1 1433814836536 ""}
{ "Info" "ITAPI_TAPI_COMPLETED" "" "Delay annotation completed successfully" {  } {  } 0 334004 "Delay annotation completed successfully" 0 0 "Quartus II" 0 -1 1433814837006 ""}
{ "Warning" "WSTA_NODE_FOUND_WITHOUT_CLOCK_ASSIGNMENT" "CLOCK_50 " "Node: CLOCK_50 was determined to be a clock but was found without an associated clock assignment." {  } {  } 0 332060 "Node: %1!s! was determined to be a clock but was found without an associated clock assignment." 0 0 "Quartus II" 0 -1 1433814837107 "|top|CLOCK_50"}
{ "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_PARENT" "" "The following clock transfers have no clock uncertainty assignment. For more accurate results, apply clock uncertainty assignments or use the derive_clock_uncertainty command." { { "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_CHILD" "altera_reserved_tck (Rise) altera_reserved_tck (Rise) setup and hold " "From altera_reserved_tck (Rise) to altera_reserved_tck (Rise) (setup and hold)" {  } {  } 1 332169 "From %1!s! to %2!s! (%3!s!)" 0 0 "Quartus II" 0 -1 1433814837109 ""} { "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_CHILD" "altera_reserved_tck (Rise) altera_reserved_tck (Fall) setup and hold " "From altera_reserved_tck (Rise) to altera_reserved_tck (Fall) (setup and hold)" {  } {  } 1 332169 "From %1!s! to %2!s! (%3!s!)" 0 0 "Quartus II" 0 -1 1433814837109 ""}  } {  } 1 332168 "The following clock transfers have no clock uncertainty assignment. For more accurate results, apply clock uncertainty assignments or use the derive_clock_uncertainty command." 0 0 "Quartus II" 0 -1 1433814837109 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "setup 45.224 " "Worst-case setup slack is 45.224" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837131 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837131 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   45.224               0.000 altera_reserved_tck  " "   45.224               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837131 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837131 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "hold 0.311 " "Worst-case hold slack is 0.311" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837138 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837138 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    0.311               0.000 altera_reserved_tck  " "    0.311               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837138 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837138 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "recovery 48.817 " "Worst-case recovery slack is 48.817" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837145 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837145 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   48.817               0.000 altera_reserved_tck  " "   48.817               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837145 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837145 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "removal 0.796 " "Worst-case removal slack is 0.796" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837152 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837152 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    0.796               0.000 altera_reserved_tck  " "    0.796               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837152 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837152 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "minimum pulse width 49.579 " "Worst-case minimum pulse width slack is 49.579" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837159 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837159 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   49.579               0.000 altera_reserved_tck  " "   49.579               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837159 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837159 ""}
{ "Info" "ISTA_REPORT_METASTABILITY_INFO" "Report Metastability: Found 5 synchronizer chains. " "Report Metastability: Found 5 synchronizer chains." { { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst-Case MTBF of Design is 1e+09 years or 3.15e+16 seconds. " "Worst-Case MTBF of Design is 1e+09 years or 3.15e+16 seconds." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Typical MTBF of Design is 1e+09 years or 3.15e+16 seconds.\n " "Typical MTBF of Design is 1e+09 years or 3.15e+16 seconds.\n" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Number of Synchronizer Chains Found: 5 " "Number of Synchronizer Chains Found: 5" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Shortest Synchronizer Chain: 3 Registers " "Shortest Synchronizer Chain: 3 Registers" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Fraction of Chains for which MTBFs Could Not be Calculated: 0.000 " "Fraction of Chains for which MTBFs Could Not be Calculated: 0.000" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst Case Available Settling Time: 198.571 ns " "Worst Case Available Settling Time: 198.571 ns" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" " " "" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst-Case MTBF values are calculated based on the worst-case silicon characteristics, with worst-case operating conditions. " "Worst-Case MTBF values are calculated based on the worst-case silicon characteristics, with worst-case operating conditions." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "  - Under worst-case conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 6.5 " "  - Under worst-case conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 6.5" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Typical MTBF values are calculated based on the nominal silicon characteristics, at nominal operating conditions. " "Typical MTBF values are calculated based on the nominal silicon characteristics, at nominal operating conditions." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "  - Under typical conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 9.9 " "  - Under typical conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 9.9" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""}  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837245 ""}
{ "Info" "0" "" "Analyzing Fast 1200mV 0C Model" {  } {  } 0 0 "Analyzing Fast 1200mV 0C Model" 0 0 "Quartus II" 0 0 1433814837254 ""}
{ "Warning" "WSTA_NODE_FOUND_WITHOUT_CLOCK_ASSIGNMENT" "CLOCK_50 " "Node: CLOCK_50 was determined to be a clock but was found without an associated clock assignment." {  } {  } 0 332060 "Node: %1!s! was determined to be a clock but was found without an associated clock assignment." 0 0 "Quartus II" 0 -1 1433814837368 "|top|CLOCK_50"}
{ "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_PARENT" "" "The following clock transfers have no clock uncertainty assignment. For more accurate results, apply clock uncertainty assignments or use the derive_clock_uncertainty command." { { "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_CHILD" "altera_reserved_tck (Rise) altera_reserved_tck (Rise) setup and hold " "From altera_reserved_tck (Rise) to altera_reserved_tck (Rise) (setup and hold)" {  } {  } 1 332169 "From %1!s! to %2!s! (%3!s!)" 0 0 "Quartus II" 0 -1 1433814837371 ""} { "Critical Warning" "WSTA_NO_UNCERTAINTY_WAS_SET_CHILD" "altera_reserved_tck (Rise) altera_reserved_tck (Fall) setup and hold " "From altera_reserved_tck (Rise) to altera_reserved_tck (Fall) (setup and hold)" {  } {  } 1 332169 "From %1!s! to %2!s! (%3!s!)" 0 0 "Quartus II" 0 -1 1433814837371 ""}  } {  } 1 332168 "The following clock transfers have no clock uncertainty assignment. For more accurate results, apply clock uncertainty assignments or use the derive_clock_uncertainty command." 0 0 "Quartus II" 0 -1 1433814837371 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "setup 47.032 " "Worst-case setup slack is 47.032" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837380 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837380 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   47.032               0.000 altera_reserved_tck  " "   47.032               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837380 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837380 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "hold 0.187 " "Worst-case hold slack is 0.187" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837390 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837390 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    0.187               0.000 altera_reserved_tck  " "    0.187               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837390 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837390 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "recovery 49.412 " "Worst-case recovery slack is 49.412" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837400 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837400 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   49.412               0.000 altera_reserved_tck  " "   49.412               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837400 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837400 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "removal 0.499 " "Worst-case removal slack is 0.499" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837408 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837408 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    0.499               0.000 altera_reserved_tck  " "    0.499               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837408 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837408 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "minimum pulse width 49.479 " "Worst-case minimum pulse width slack is 49.479" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack       End Point TNS Clock  " "    Slack       End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837414 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= =================== ===================== " "========= =================== =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837414 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   49.479               0.000 altera_reserved_tck  " "   49.479               0.000 altera_reserved_tck " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837414 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1433814837414 ""}
{ "Info" "ISTA_REPORT_METASTABILITY_INFO" "Report Metastability: Found 5 synchronizer chains. " "Report Metastability: Found 5 synchronizer chains." { { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst-Case MTBF of Design is 1e+09 years or 3.15e+16 seconds. " "Worst-Case MTBF of Design is 1e+09 years or 3.15e+16 seconds." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Typical MTBF of Design is 1e+09 years or 3.15e+16 seconds.\n " "Typical MTBF of Design is 1e+09 years or 3.15e+16 seconds.\n" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Number of Synchronizer Chains Found: 5 " "Number of Synchronizer Chains Found: 5" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Shortest Synchronizer Chain: 3 Registers " "Shortest Synchronizer Chain: 3 Registers" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Fraction of Chains for which MTBFs Could Not be Calculated: 0.000 " "Fraction of Chains for which MTBFs Could Not be Calculated: 0.000" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst Case Available Settling Time: 199.123 ns " "Worst Case Available Settling Time: 199.123 ns" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" " " "" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Worst-Case MTBF values are calculated based on the worst-case silicon characteristics, with worst-case operating conditions. " "Worst-Case MTBF values are calculated based on the worst-case silicon characteristics, with worst-case operating conditions." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "  - Under worst-case conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 6.5 " "  - Under worst-case conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 6.5" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "Typical MTBF values are calculated based on the nominal silicon characteristics, at nominal operating conditions. " "Typical MTBF values are calculated based on the nominal silicon characteristics, at nominal operating conditions." {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""} { "Info" "ISTA_REPORT_METASTABILITY_INFO" "  - Under typical conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 9.9 " "  - Under typical conditions, an increase of 100ps in available settling time will increase MTBF values by a factor of 9.9" {  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""}  } {  } 0 332114 "%1!s!" 0 0 "Quartus II" 0 -1 1433814837501 ""}
{ "Info" "ISTA_UCP_NOT_CONSTRAINED" "setup " "Design is not fully constrained for setup requirements" {  } {  } 0 332102 "Design is not fully constrained for %1!s! requirements" 0 0 "Quartus II" 0 -1 1433814837661 ""}
{ "Info" "ISTA_UCP_NOT_CONSTRAINED" "hold " "Design is not fully constrained for hold requirements" {  } {  } 0 332102 "Design is not fully constrained for %1!s! requirements" 0 0 "Quartus II" 0 -1 1433814837661 ""}
{ "Info" "IQEXE_ERROR_COUNT" "TimeQuest Timing Analyzer 0 s 12 s Quartus II 64-Bit " "Quartus II 64-Bit TimeQuest Timing Analyzer was successful. 0 errors, 12 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "528 " "Peak virtual memory: 528 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "Quartus II" 0 -1 1433814837786 ""} { "Info" "IQEXE_END_BANNER_TIME" "Tue Jun 09 09:53:57 2015 " "Processing ended: Tue Jun 09 09:53:57 2015" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "Quartus II" 0 -1 1433814837786 ""} { "Info" "IQEXE_ELAPSED_TIME" "00:00:02 " "Elapsed time: 00:00:02" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "Quartus II" 0 -1 1433814837786 ""} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:02 " "Total CPU time (on all processors): 00:00:02" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "Quartus II" 0 -1 1433814837786 ""}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "Quartus II" 0 -1 1433814837786 ""}
